Technical specification of the raw data of PRISME DOOR programme
Author: W. LE SAUX
Date:  June 2007

1. RAW DATA
-----------
The names of the sensors are indicated for each test directory in the files “Output_PRS_D*.txt (*=1 to 6)”. 

Their characteristics are detailed in the reports [1] to [7].

For a test, raw data have all the same time vector which is normalized with a constant time step.

The zero value of the time vector corresponds to ignition time identified for each test.

These times (in s) are recalled below:

 ____________________________________________________
|PRS_D1 | PRS_D2 | PRS_D3 | PRS_D4 | PRS_D5 | PRS_D6 |
|-------|--------|--------|--------|--------|--------|
|  865  |  902   |  950	  |  920   |  660   |  790   |
|_______|________|________|________|________|________|

      Table 1: Start of the fire for the tests.

Sensors using a sampling system show a time lag because of the sampling process.

This time delays are not taken into account in these raw data.

The definitive data will be available after the issue of the PRISME DOOR Analysis report.


2.	FORMAT
--------------
For each test, six ASCII data files (room1.data, room2.data, room3.data, door.data, target.data and ventil.data) are located in a directory sharing the name of the test
PRS_D* (* stands for the test number).


