COMPUTED DATA
---------------
All the computed data are obtained from raw data. 

For each test, computed data ASCII files are located in a directory sharing the name of the test
PRS_D* (* stands for the test number).

Those files, which first column is the time vector (which zero value corresponds to ignition),
are containing the numerical values corresponding to the curves and the figure keys presented in
the PRISME DOOR Analysis Report (DPAM/SEREA-2008-157; PRISME 27).
They contain the following computed data :

- Fuel mass loss rate (MLR)
- Heat release rates (HRR - mechanical, chemical O2, chemical CO2 and thermal)
- Mass concentrations of species (Y_O2, Y_CO2, Y_CO and Y_THC)
- Soot mass rates extracted from Excell TEOM files (TEOM_'test name'.txt) 
- Volumetric flow rates at the door(s)
- Mass rates at the door(s)
- Net heat rates at the door(s)
- Neutral planes at the door(s)
- Heat absorption rates in the PVC rods.

Revision 1 (Data and charts) :
- Height of interface between lower zone and upper zone
- Upper and lower temperatures
